ITEM #: REVERSE OSMOSIS SYSTEM  
Quantity: One (1)  
Manufacturer: WaterSpec  
Model No.: 310062 (RO250NE)  
Pertinent Data: For Item #  
Utilities Req’d: 3/8” CW, 1/4” IW

See plans for location and placement of item with reference to adjoining equipment.   
Furnish and set in place per manufacturer’s standard specifications and the following:  
1. Set in place in location as shown on drawings.  
2. Size and configuration as shown on drawings.  
3. Coordinate installation with Item #, Reverse Osmosis Water Storage Tank.  
4. Provide components that are contained in a plastic enclosure with bulk head fittings, built in bypass and TDS bleed valve facilitating installation and initial system setup.  
5. Provide incorporation of a Permeate Pump that ensures excellent performance guarantying lowest product water / waste water ratio possible. ScaleS tick insert inside primary cartridge extends membrane life and improves performance.  
6. Provide a built in TDS Meter that allows the user to monitor RO system performance by reading the incoming and outgoing TDS of the water.  
7. Must meet all applicable federal, state, and local laws, rules, regulations, and codes.