ITEM #: ROLL-IN COMBI OVEN  
Quantity: One (1)  
Manufacturer: Rational  
Model No.: SCC 202 E  
Pertinent Data: Floor Model  
Utilities Req'd: 208V/3PH, 189.0A; 3/4” CW, 3/4” R.O.  
  
See plans for location and placement of item with reference to adjoining equipment.  
Furnish and set in place per manufacturer's standard specifications and the following:  
1. Set in place in location as shown on drawings.  
2. Size and configuration as shown on drawings.  
3. Provide LED cooking cabinet and rack lighting - energy-saving, durable and low maintenance.  
4. Provide rear-ventilated triple-pane cooking cabinet door, two hinged inside panes (for easy cleaning) with a special heat-reflecting coating.  
5. Provide integrated Ethernet and USB port to connect to a cloud based system for administration of cooking processes, management of HACCP and service data and remote control.  
6. Provide individual programming of at least 1,200 cooking programs with up to 12 steps transferable via USB.  
7. Equip unit with a hand shower with automatic retracting system.  
8. Provide integral, maintenance-free grease extraction system.  
9. Include a single water connection as shipped, can be split connection for treated and untreated water.  
10. Provide five programmable proofing stages.  
11. Provide the unit with Delta-T Cooking.  
12. Equip unit with digital, graphically supported overview of the current cooking chamber climate, review and forecast as well as repeat and change options at the end of the cooking process.  
13. Unit shall have a remote control function using software and mobile app.  
14. Unit shall include a self-learning operation, automatically adapts to actual usage.  
15. Provide the unit with installation kits.  
16. Provide preventative maintenance kits.  
17. Must meet all applicable federal, state, and local laws, rules, regulations, and codes.