ITEM #: ROLL-IN PROOFER  
Quantity: One (1)  
Manufacturer: Gemini  
Model No.: GRP 1  
Pertinent Data: Single Rack  
Utilities Req’d: 208V/3PH; 20.0A; 15mm CW, 15mm IW  
  
See plans for location and placement of item with reference to adjoining equipment.   
Furnish and set in place per manufacturer’s standard specifications and the following:  
1. Set in place in location as shown on drawings.  
2. Size and configuration as shown on drawings.  
3. Proofer shall be provided with one (1) single rack capacity.  
4. The proofer shall be constructed of heavy-duty stainless steel, and aluminized top.  
5. Provide the proofer with a stainless steel floor.  
6. The proofer all digital controls mounted in the door at eye level.  
7. Equip the unit with PID Type controls for rapid accurate response without overshoot.  
8. Proofer shall have a rapid responding air wash heat and humidity system.  
9. Proofer controls shall contain a digital set Temperature, Humidity, Time.  
10. Proofer shall be provided with large LED displays.  
11. Must meet all applicable federal, state, and local laws, rules, regulations, and codes.