ITEM #: ROLL-IN RACK OVEN  
Quantity: One (1)  
Manufacturer: Gemini  
Model No.: C152  
Pertinent Data: ---  
Utilities Req’d: 120V/1PH; 15.0A; 3/4” LP Gas @ 175,000 BTUs; 5.5” WC; 3/8” CW; 3/8” IW  
  
See plans for location and placement of item with reference to adjoining equipment.   
Furnish and set in place per manufacturer’s standard specifications and the following:  
1. Set in place in location as shown on drawings.  
2. Size and configuration as shown on drawings.  
3. Equip unit with a control panel which can be operated both manually or is programmable up to 99 recipes.  
4. Unit shall be provided with all stainless steel construction and approved for zero clearance to combustible surfaces sides, and rear.  
5. Provide unit with the patented cascade steam system.  
6. Equip unit with a door latch design completely in stainless material and with double lock cylinders.  
7. Unit shall be equipped with a front drain.  
8. Provide unit with a Type I Hood and Grease Filters, with single point connection for roasting.  
9. Equip unit with electric A Soft Start” rack rotation.  
10. Unit shall be supplied with a Door/Exhaust Fan interlock.  
11. Must meet all applicable federal, state, and local laws, rules, regulations, and codes.