ITEM #: ROLL-IN REFRIGERATOR  
Quantity: One (1)  
Manufacturer: True  
Model No.: STA1RRI-1S  
Pertinent Data: Single Section, Self-Contained  
Utilities Req’d: 120V/1PH; 8.9A

See plans for location and placement of item with reference to adjoining equipment.  
Furnish and set in place per manufacturer’s standard specifications and the following:  
1. Set in place in location as shown on drawings.  
2. Provide stainless steel door, front and sides on the exterior, and aluminum sides, wall and back on the interior.  
3. Provide heavy-duty cord and plug, coordinate NEMA configuration with Electrical Contractor.  
4. Provide top mounted compressor.  
5. Provide LED lights with proximity door switch activates interior lighting.  
6. Provide removable door ramps.  
7. Must meet all applicable federal, state, and local laws, rules, regulations, and codes.