ITEM #: ROLL-THRU REFRIGERATOR  
Quantity: One (1)  
Manufacturer: True Food Service Equipment  
Model No.: STA-2RRT-2G-2S  
Pertinent Data: Self-Contained  
Utilities Req’d: 120V/1PH; 9.5A  
  
See plans for location and placement of item with reference to adjoining equipment.  
Furnish and set in place per manufacturer’s standard specifications and the following:  
1. Set in place in location as shown on drawings.  
2. Size and configuration as shown on drawings.  
3. Provide two (2) glass doors on the Servery side of the unit and two (2) solid doors on the Pot/Pan Wash side of the refigerator.  
4. Provide stainless steel sides, front and back on the exterior, and aluminum side walls with stainless steel floor and ceiling on the interior.  
5. Provide four heavy gauge stainless steel roll-in ramps one for each door.  
6. Provide incandescent interior lighting safety shielded.  
7. Must meet all applicable federal, state, and local laws, rules, regulations, and codes.