ITEM #: ROTISSERIE WITH HEATED CABINET  
Quantity: One (1)  
Manufacturer: Rostisol France Inc.  
Model No.: 1350/5  
Pertinent Data: ---  
Utilities Req’d: 208V/1PH, 5.2A; 3/4" Gas @ 28,000 BTU’s; 5" WC

See plans for location and placement of item with reference to adjoining equipment.  
Furnish and set in place per manufacturer’s standard specifications and the following:  
1. Set in place in location as shown on drawings.  
2. Provide unit with middle drip pan.   
3. Provide unit with heated base cabinet on four (4) heavy duty, polyurethane casters, two (2) with brakes.  
4. Provide unit with 5 chicken spit.   
5. Provide unit with bottom drip pan with drain plug.   
6. Provide unit with tempered glass doors.   
7. Provide unit with 5 adjustable spits.   
8. Provide unit with powerful halogen light.   
9. Provide unit with retractable table.   
10. Provide heavy-duty cord and plug, coordinate NEMA configuration with Electrical Contractor.  
11. Must meet all applicable federal, state, and local laws, rules, regulations, and codes.