ITEM #: SALAD DRYER  
Quantity: One (1)  
Manufacturer: Nilma  
Model No.: IDROVER 50  
Pertinent Data: ---  
Utilities Req’d: 208V/3PH; 3.4A; 2” IW  
  
See plans for location and placement of item with reference to adjoining equipment.   
Furnish and set in place per manufacturer’s standard specifications and the following:  
1. Set in place in location as shown on drawings.  
2. Size and configuration as shown on drawings.  
3. Provide unit with an outer case made of satin finish stainless steel 18/10.  
4. Equip unit with a shock proof alimentary plastic hinged cover.  
5. Unit shall be equipped with a lid safety locking device with timed automatic opening/closing.  
6. Provide an aluminum alloy base with holes for fixing to the floor.  
7. Equip the unit with a self-balanced removable basket made of satin finish stainless steel 18/10.  
8. Unit shall be equipped with a counter basket made of satin finish stainless steel 18/10 removable for cleaning.  
9. Equip unit with a self-braking motor.  
10. Provide a wall control board equipped with start/stop push button, lid locking warning light, and a 4” timer.  
11. Must meet all applicable federal, state, and local laws, rules, regulations, and codes.