ITEM #: SANDWICH / SALAD PREPARATION REFRIGERATOR  
Quantity: One (1)  
Manufacturer: True Food Service Equipment  
Model No.: TSSU-60-24M-B-ST-ADA-FGLID-HC  
Pertinent Data: Self-Contained  
Utilities Req’d: 120V/ 1PH, 6.5A

See plans for location and placement of item with reference to adjoining equipment.  
Furnish and set in place per manufacturer’s standard specifications and the following:  
1. Set in place in location as shown on drawings.  
2. Provide self-contained refrigeration system.  
3. Provide two (2) stainless steel exterior refrigerator doors with white aluminum liner to match interior of unit.  
4. Provide recessed handles on door.  
5. Provide the unit with barrel locks for each door.  
6. Provide 8-7/8" deep x 1/2" thick polyethylene cutting board.  
7. Provide 24 pan capacity refrigerated rail with pan dividers.  
8. Provide stainless steel foam insulated flat lid.  
9. Equip unit with factory installed exterior rectangular digital temperature display.  
10. Provide unit with 3" diameter, heavy duty, polyurethane, casters, two (2) with brakes.   
11. Coordinate installation with Item #  
12. Must meet all applicable federal, state, and local laws, rules, regulations, and codes.