ITEM #: SELF-SERVICE REFRIGERATED MERCHANDISER  
Quantity: One (1)  
Manufacturer: True Food Service Equipment  
Model No.: GDM-35-HC  
Pertinent Data: Self-Contained, Double Section  
Utilities Req'd: 120V/1PH: 6.5A

See plans for location and placement of item with reference to adjoining equipment.  
Furnish and set in place per manufacturer's standard specifications and the following:  
1. Set in place in location as shown on drawings.  
2. Size and configuration as shown on drawings.  
3. Provide exterior to be non-peel or chip black powder coated cold rolled steel; durable and permanent.  
4. Provide interior of attractive, NSF approved, white aluminum interior liner with stainless steel floor.  
5. Equip unit with front doors which shall be self-closing solid swing doors. Positive seal, torsion type closure system.  
6. Equip unit with rear doors which shall be self-closing solid swing doors. Positive seal, torsion type closure system.  
7. Provide ALow-E@, double pane thermal insulated glass door assemblies with mitered plastic channel frames.  
8. Unit shall be equipped with LED interior lighting provides more even lighting throughout the cabinet. Safety shielded.  
9. Provide unit with 2-1/2" diameter Casters.  
10. Provide unit with heavy duty cord and plug, coordinate NEMA configuration with electrical contractor.  
11. KEC shall provide trim strips between the wall opening and the Refrigerator.  
12. Must meet all applicable federal, state, and local laws, rules, regulations, and codes.