ITEM #: SIX BURNER RANGE  
Quantity: One (1)  
Manufacturer: Jade  
Model No.: JTRH-6-36  
Pertinent Data: ---  
Utilities Req’d: 3/4” Gas @ 245,000 BTU’s; 5” WC  
  
See plans for location and placement of item with reference to adjoining equipment.   
Furnish and set in place per manufacturer’s standard specifications and the following:  
1. Set in place in location as shown on drawings.  
2. Size and configuration as shown on drawings.  
3. Provide 3/4” rear gas connection, cap and cover front gas manifold on both left and right side.  
4. Provide six individual lift off grates.  
5. Provide four (4) 6” high adjustable heavy-duty, non-marking casters, two (2) with brakes.  
6. Provide cast iron design features flame shaping center tube for more efficient heat transfer.  
7. Equip unit with a stainless steel 6” plate shelf.  
8. To have conventional oven base with stainless steel lining. Oven sides and bottom to be removable without tools. Provided with two oven racks. Thermostat to adjust from 150°F to 550°F with 35,000 BTU burner. Oven interior 28-1/4" W x 14" H x 27-3/4" D.  
9. Provide 14-gauge stainless steel interior sides rear and deck on oven.  
10. Provide 48” flex, quick disconnect gas hose with restraining device and gas pressure regulator.  
11. Provide Posi-Set.  
12. Must meet all applicable federal, state, and local laws, rules, regulations, and codes.