ITEM #: SIX BURNER RANGE  
Quantity: One (1)  
Manufacturer: Jade  
Model No.: JTRH-6-36C  
Pertinent Data: ---  
Utilities Req’d: 120V/1PH, 4.0A; 3/4” Gas @ 240,000 BTU’s; 5” WC

See plans for location and placement of item with reference to adjoining equipment.   
Furnish and set in place per manufacturer’s standard specifications and the following:  
1. Set in place in location as shown on drawings.  
2. Size and configuration as shown on drawings.  
3. Provide a convection oven with a high-performance stainless steel unique burner at 30,000 BTU’s.  
4. Provide Six individual lift off grates.  
5. Provide four (4) 6” high adjustable heavy-duty, non-marking casters, two (2) with brakes.  
6. Provide cast iron design features flame shaping center tube for more efficient heat transfer.  
7. Equip unit with a stainless steel 6” plate shelf.  
8. To have convection base with 14 gauge stainless steel interior. Provide with two oven racks. Thermostat to adjust from 150°F to 550°F with 30,000 BTU burner. Provided with 1/4 HP 115/60/1 blower motor. Oven interior 28" W x 13-3/4" H x 24-1/2" D.  
9. Provide 14-gauge stainless steel interior sides rear and deck on oven.  
10. Provide 48” flex, quick disconnect gas hose with restraining device and gas pressure regulator.  
11. Provide Posi-Set.  
12. Must meet all applicable federal, state, and local laws, rules, regulations, and codes.