ITEM #: SLICER  
Quantity: One (1)  
Manufacturer: Globe  
Model No.: S13A  
Pertinent Data: Automatic  
Utilities Req’d.: 120V/1PH, 2.5A

See plans for location and placement of item with reference to adjoining equipment.   
Furnish and set in place per manufacturer’s standard specifications and the following:  
1. Set in place in location as shown on drawings.  
2. Provide unit with belt drive system.  
3. Provide unit with easy movement with smooth stainless steel ball bearing chute slide.  
4. Provide unit with 13” hard chromed special alloy, hollow ground knife.  
5. Provide unit with anodized aluminum construction with seamless edges and radius corners.  
6. Provide sealed splash zones for added sanitation and protection of electronics.  
7. Provide with heavy-duty cord and plug, coordinate NEMA configuration with Electrical Contractor.  
8. Must meet all applicable federal, state, and local laws, rules, regulations, and codes.