ITEM #: SMOKEHOUSE BBQ PIT  
Quantity: One (1)  
Manufacturer: J & R Manufacturing  
Model No.: 250FSE  
Pertinent Data: Solid Fuel  
Utilities Req’d: 208V/1PH; 18.3A  
  
See plans for location and placement of item with reference to adjoining equipment.  
Furnish and set in place per manufacturer’s standard specifications and the following:  
1. Set in place in location as shown on drawings.  
2. Size and configuration as shown on drawings.  
3. Provide a capacity of 250 pounds of heavy meat or 50 slabs of ribs capacity per load.  
4. Provide easy fire starting with built-in stack fan providing draft and the combustion air fan providing oxygen.  
5. Provide an evacuation system of damper and fan system to induce fresh air into the pit.  
6. Provide the unit with a cook and hold system.  
7. Provide removable racks and rack slides, a large drain valve, and easy to reach walls in a stainless steel interior for cleaning.  
8. Must meet all applicable federal, state, and local laws, rules, regulations, and codes.