ITEM #: SNEEZE GUARD WITH LIGHTS  
Quantity: One (1)  
Manufacturer: VersaGard  
Model No.: Europa  
Pertinent Data: ---  
Utilities Req’d: 120V/1PH; 2.0A

See plans for location and placement of item with reference to adjoining equipment.   
Fabricate and set in place per plans, details, and the following:  
1. Set in place in location as shown on drawing.  
2. Provide unit with 6.3mm bent front tempered glass with left and right side end panels.  
3. Provide unit with black powder coated supports verify with the Architect and or Interior Designer the color.  
4. Provide 1” radius on all corners.  
5. Coordinate installation of slim line LED lights.  
6. Unit shall be fabricated to meet NSF/ANSI 2 2010 Standards Requirements.  
7. Coordinate installation over Item #, Refrigerated Sandwich Station, and Item #, Hot Food Well.  
8. Provide FL17.1A concealed mount to counter top.  
9. Provide shop drawings prior to fabrication.  
10. Must meet all applicable federal, state, and local laws, rules, regulations, and codes.