ITEM #: SNEEZE GUARD  
Quantity: One (1)  
Manufacturer: BSI  
Model No.: ZG9930  
Pertinent Data: Slim Light  
Utilities Req’d: 120V/1PH; 2.0A  
  
See plans for location and placement of item with reference to adjoining equipment.   
Fabricate and set in place per plans, details, and the following:  
1. Set in place in location as shown on drawing.  
2. Provide unit with 1/4” tempered front adjustable glass.  
3. Provide unit with 3/8” tempered top glass.  
4. Provide 1” radius on all corners.  
5. Sneeze guard shall be provided for dual service, self-service, and full service.  
6. Provide slim line LED light fixture.  
7. All supports and base shall be 1” diameter and shall extend into the counter for support.  
8. All finishes shall be NSF listed and certified. Verify finishes with the Interior Designer.  
9. Coordinate installation over Item #, Service Counter With Sink.  
10. Provide under counter mount.  
11. Provide shop drawings prior to fabrication.  
12. Must meet all applicable federal, state, and local laws, rules, regulations, and codes.