ITEM #: SOILED DISHTABLE  
Quantity: One (1)  
Manufacturer: Custom Fabrication  
Model No.: Stainless Steel  
Pertinent Data: See Plans, Drawing #FS  
Utilities Req’d:   
  
See plans for location and placement of item with reference to adjoining equipment.   
Fabricate and set in place per plans, details, and the following:  
1. Standard fabrication Drawing #FSX.X, Detail #1A, #2B, #4C, #5A, #15, #45, #46, and #48.  
2. Set in place in location as shown on drawings.  
3. Size and configuration as shown on drawings.  
4. Provide flanged feet on front legs to secure to floor.  
5. Provide fully enclosed corner and 3/4” turndown at Item #, Dish Machine.  
6. Provide 16 gauge stainless steel undershelf with 2” turn up at rear.  
7. Provide a fully enclosed backsplash and a fully enclose rolled edge. Provide a cutout for Item #, Food Waste Collector.  
9. Provide Stainless steel bracket for Item #, Food Waste Collector controls.  
10. Coordinate fabrication and installation with Item #, PassThru Dish Drop Window.  
11. KEC shall provide 22 gauge stainless steel flashing from top of splash to up at least 84” AFF.  
12. Provide space under table for Item #, Trash Receptacle.  
13. Fabricate unit utilizing security prison procedures.  
14. Provide shop drawings for approval prior to fabrication.  
15. Must meet all applicable federal, state, and local laws, rules, regulations, and codes.