ITEM #: SOUS VIDE IMMERSION CIRCULATOR  
Quantity: One (1)  
Manufacturer: PolyScience  
Model No.: Sous Vide ProfessionalJ Classic Series   
Pertinent Data: ---  
Utilities Req’d: 208V/1PH; 7.7A  
  
See plans for location and placement of item with reference to adjoining equipment.   
Furnish and set in place per manufacturer’s standard specifications and the following:  
1. Set in place in location as shown on drawings.  
2. Size and configuration as shown on drawings.  
3. Provide a double wall stainless steel tank with convenient drain valve.  
4. Provide a controller mounted to a bridge which can easily be removed for cleaning.  
5. Provide with a generous bath opening provides easy access to food.  
6. Must meet all applicable federal, state, and local laws, rules, regulations, and codes.