ITEM #: SPREADER CABINET  
Quantity: One (1)  
Manufacturer: Jade  
Model No.:   
Pertinent Data: ---  
Utilities Req’d: ---  
  
See plans for location and placement of item with reference to adjoining equipment.   
Furnish and set in place per manufacturer’s standard specifications and the following:  
1. Set in place in location as shown on drawings.  
2. Size and configuration as shown on drawings.  
3. Unit shall have a 14-gauge stainless steel all welded body construction.  
4. Provide stainless steel top, front, sides and stub back.  
5. Equip unit with stainless steel 6” plate shelf.  
6. Provide insulated double wall doors.  
7. Provide four (4) 6” high adjustable heavy-duty, non-marking casters, two (2) with brakes.  
8. Must meet all applicable federal, state, and local laws, rules, regulations, and codes.