ITEM #: STOCK POT RANGE  
Quantity: One (1)  
Manufacturer: Jade Range  
Model No.: JSP-182  
Pertinent Data: Mobile  
Utilities Req’d: 3/4” Gas @ 90,000 BTU’s, 5” WC

See plans for location and placement of item with reference to adjoining equipment.   
Furnish and set in place per manufacturer’s standard specifications and the following:  
1. Set in place in location as shown on drawings.  
2. Size and configuration as shown on drawings.  
3. Provide unit with two (2) three stage steel open burners.  
4. Provide Infinite control manual gas valves at each burner ring for precise heat control.  
5. Unit shall be provided with stainless steel front, plate shelf and sides with welded and finished seams.  
6. Provide stainless steel tubing throughout.  
7. Provide 48” flex, quick disconnect gas hose with restraining device and gas pressure regulator.  
8. Provide Posi-Set.  
9. Provide four (4) heavy-duty, non-marking casters, two (2) with brakes.  
10. Must meet all applicable federal, state, and local laws, rules, regulations, and codes.