ITEM # : SUSHI CASE  
Quantity: One (1)  
Manufacturer: Apice Cooling Technology  
Model No.: Stainless Steel  
Pertinent Data: See Plans, Drawing #FS  
Utilities Req’d: 120V/1PH; 8.0A OR 230V/1PH, 1.15KW  
  
See plans for location and placement of item with reference to adjoining equipment.  
Fabricate and set in place per plans, details, and the following:  
1. See Custom Fabrication Drawing #\_\_\_\_\_\_\_\_  
2. Set in place in location as shown on drawings.  
3. Size and configuration as shown on drawings.  
4. Equip unit with NSF approved thermometer.  
5. Provide plate space on top of unit.  
6. Coordinate installation onto Item #\_\_\_\_\_\_\_\_\_  
7. Condensing unit to be located in Item #\_\_\_, Refrigeration Rack. Unit to consist of all components necessary for a fully functioning system.   
8. Unit shall have larger front to back interior 279.4mm (11").  
9. Equip unit with large diameter upper evaporator with tin plating.  
10. Provide slightly taller doors with plastic seal at end, opposite of the handle.  
11. Provide slanted front display window.  
12. Equip with double paned heated glass.  
13. Provide shop drawings for approval prior to fabrication.  
14. Must meet all applicable federal, state, and local laws, rules, regulations, and codes.