ITEM #521: THREE COMPARTMENT SINK  
Quantity: One (1)  
Manufacturer: Perlick  
Model No.: TSF48M3-DBL  
Pertinent Data: ---  
Utilities Req’d: (2) 1/2" HW, (2)1/2" CW, (4) 1-1/2" IW  
  
See plans for location and placement of item with reference to adjoining equipment.  
Furnish and set in place per manufacturer’s standard specifications and the following:  
1. Set in place in location as shown on drawings.  
2. Size and configuration as shown on drawings.  
3. Provide unit with three (3) 18-gauge stainless steel compartments with 10" x 14" x 9.25" stainless steel bowls with under coating to absorb sound.  
4. Provide 12" pitched drainboard top on left and right.  
5. Unit shall have 1-5/8" OD stainless steel legs shrouded with stainless steel to conceal the legs.  
6. Provide unit with 926-10LF Lead Free Faucet, deck-mounted, nominal 4" centers, swing nozzle, 10" long nozzle.  
7. Provide unit with a 6" high backsplash with a 1" return at the top.  
8. Provide shop drawings for approval prior to fabrication.  
9. Must meet all applicable federal, state, and local laws, rules, regulations, and codes.