ITEM #: TOASTER  
Quantity: One (1)  
Manufacturer: Hatco  
Model No.: TPT-120  
Pertinent Data: Pop-Up  
Utilities Req’d: 120V/1PH; 15.0A

See plans for location and placement of item with reference to adjoining equipment.   
Furnish and set in place per manufacturer’s standard specifications and the following:  
1. Set in place in location as shown on drawings.  
2. Equip unit with four (4) 1-1/4” wide self-centering slots.  
3. Provide manual controls.  
4. Unit shall be equipped with a removable crumb tray.  
5. Provide with heavy-duty cord and plug. Coordinate NEMA configuration with Electrical Contractor.  
6. Equip unit with stainless steel construction and finish.  
7. Must meet all applicable federal, state, and local laws, rules, regulations, and codes.