ITEM #: TWO BURNER STOCK RANGE  
Quantity: One (1)  
Manufacturer: Imperial  
Model No.: ISPA182E  
Pertinent Data: Mobile  
Utilities Req’d: 208V/3PH; 44.0A  
  
See plans for location and placement of item with reference to adjoining equipment.   
Furnish and set in place per manufacturer’s standard specifications and the following:  
1. Set in place in location as shown on drawings.  
2. Size and configuration as shown on drawings.  
3. Provide unit with two (2) three ring burners.  
4. Provide dual controls per coil.  
5. Unit shall be provided with stainless steel front, and side with welded and finished seams.  
6. Provide a stainless steel cabinet base for storage.  
7. Equip the unit with knobs that are cast aluminum with Vylox heat protection grip.  
8. Provide four (4) heavy-duty, non-marking casters, two (2) with brakes.  
9. Must meet all applicable federal, state, and local laws, rules, regulations, and codes.