ITEM #: UNDERBAR DRAFT BEER COOLER  
Quantity: One (1)  
Manufacturer: True Food Service Equipment   
Model No.: TDD-4S-HC  
Pertinent Data: Self-Contained  
Utilities Req’d: 120V/1PH; 2.8A; 1" IW

See plans for location and placement of item with reference to adjoining equipment.  
Furnish and set in place per manufacturer’s standard specifications and the following:  
1. Set in place in location as shown on drawings.  
2. Size and configuration as shown on drawings.  
3. Keg Cooler shall be self-contained refrigeration with the condensing unit on the left.  
4. Unit shall be provided with heavy duty cord and plug, coordinate NEMA configuration with electrical contractor.  
5. Provide stainless steel doors field reversible hinged left, left, left, left.  
6. Unit shall have the door threshold with reinforced lip.  
7. Provide unit with 2-1/2”casters.  
9. Coordinate installation of two 3” diameter stainless steel insulated beer columns.  
10. Unit shall have a four 1/2 barrel capacity.  
11. Must meet all applicable federal, state, and local laws, rules, regulations, and codes.