ITEM #: UNDERCOUNTER GLASS WASHER  
Quantity: One (1)  
Manufacturer: Champion  
Model No.: UH230B  
Pertinent Data: Single Tank  
Utilities Req’d: 208V/1PH; 32.0A; 1/2” CW; 1/2” IW  
  
See plans for location and placement of item with reference to adjoining equipment.   
Furnish and set in place per manufacturer’s standard specifications and the following:  
1. Set in place in location as shown on drawings.  
2. Unit shall be provided with built-in 39 degree C rise (70 degree F rise) booster heater.  
3. Unit shall be provided StemSure soft start to protect glasses and dishes from chipping and breaking.  
4. Unit shall be provided with Rinse Sentry which extends the cycle time to ensure 180⁰F/82⁰C final rinse.  
5. Provide shop drawings for approval prior to installation.  
6. Must meet all applicable federal, state, and local laws, rules, regulations, and codes.