ITEM #: UNDERCOUNTER ICE MACHINE WITH BIN  
Quantity: One (1)  
Manufacturer: Scotsman  
Model No.: CU50PA-1  
Pertinent Data: 49 Pounds ARI Capacity, Air Cooled  
Utilities Req’d: 120V/1PH, 15.0A; 1/4" CW, 5/8" IW  
  
See plans for location and placement of item with reference to adjoining equipment.  
Furnish and set in place per manufacturer’s standard specifications and the following:  
1. Set in place in location as shown on drawings.  
2. Unit shall be all stainless steel construction.  
3. Coordinate with Plumbing Contractor on the connection between ice maker and Item #\_\_\_\_\_, Water Filtration System.  
4. Install ice maker under Item #\_\_\_\_\_, Work Counter with Sink.  
5. Ice maker shall produce gourmet ice 1” x 1-1/8” x 1-1/4”.  
6. Provide unit with a control board, a water sensor and a scoop.  
7. Must meet all applicable federal, state, and local laws, rules, regulations, and codes.