ITEM #: UNDERCOUNTER ICE MACHINE  
Quantity: One (1)  
Manufacturer: Scotsman  
Model No.: CU50GA-1  
Pertinent Data: Self Contained, Air Cooled  
Utilities Req’d: 120V/1PH; 15.0A; 3/8" CW; 5/8" IW

See plans for location and placement of item with reference to adjoining equipment.  
Furnish and set in place per manufacturer’s standard specifications and the following:  
1. Set in place in location as shown on drawings.  
2. Size and configuration as shown on drawings.  
3. Provide a water-quality sensor which detects hard water conditions and control system purges mineral laden water with every harvest cycle, which helps extend the time between cleanings.  
4. Provide a user-friendly control panel that informs whether power is on, alerts a no-water condition, and a time to clean reminder.  
5. Coordinate installation under Item #\_\_\_\_\_, Beverage Counter with Sink.  
6. Coordinate with Plumbing Contractor on the connection between ice maker and Item #\_\_\_\_\_, Water Filtration System.  
7. Must meet all applicable federal, state, and local laws, rules, regulations, and codes.