ITEM # : UNDERCOUNTER ICE MACHINE  
Quantity: One (1)  
Manufacturer: Scotsman  
Model No.: UF0915  
Pertinent Data: 76 Lbs. Capacity, Air Cooled  
Utilities Req’d: 120V/1PH,15.2A; 1/4" CW, 3/4" IW  
  
See plans for location and placement of item with reference to adjoining equipment.  
Furnish and set in place per manufacturer’s standard specifications and the following:  
1. Set in place in location as shown on drawings.  
2. Size and configuration as shown on drawings.  
3. Unit shall be front breathing with no side clearance required.  
4. Provide floor mount kit allows for installation under 34“ ADA counter tops.  
5. Equip with unit specific QR code for quick access to service manuals, cleaning guides and warranty history.  
6. Provide ergonomic slide back door allows easy access to ice in the bin.  
7. Provide with heavy-duty cord and plug, coordinate NEMA configuration with Electrical Contractor.  
8. Equip with sealed, maintenance-free bearings for reduced preventative maintenance and long-lasting performance.  
9. Provide stainless-steel evaporator and auger for maximum durability.  
10. Unit shall have a heavy duty, rust-free front panel and corrosion-resistant aluminum alloy side panels for maximum lifespan  
11. Provide the connection between ice machine and Item #\_\_\_\_\_, Water Filtration System.  
12. Must meet all applicable federal, state, and local laws, rules, regulations, and codes.