ITEM #: UNDERCOUNTER ICE MAKER  
Quantity: One (1)   
Manufacturer: Scotsman  
Model No.: CU3030MA-1  
Pertinent Data: 245 LBS Capacity, Air Cooled  
Utilities Req’d: 120V/1PH, 15.0A; 3/8" CW, 3/4" IW  
  
See plans for location and placement of item with reference to adjoining equipment.  
Furnish and set in place per manufacturer’s standard specifications and the following:  
1. Set in place in location as shown on drawings.  
2. Unit shall be all stainless steel construction.  
3. Coordinate the connection between ice maker and Item #\_\_\_\_\_, Water Filtration System.  
4. Install ice maker under Item #\_\_\_\_\_, Back Serving Counter with Sink, and coordinate proper installation.  
5. Ice maker shall produce dice cubes 7/8" by 7/8" by 7/8" thick.  
6. Provide bin with 110 lbs. ice storage capacity.  
7. Provide 6" stainless steel legs.  
8. Provide slide up and in bin door.  
9. Must meet all applicable federal, state, and local laws, rules, regulations, and codes.