ITEM #: UNDERCOUNTER ICE MAKER  
Quantity: One (1)  
Manufacturer: Scotsman  
Model No.: CU3030MA-1A  
Pertinent Data: 300 Pounds Capacity, Air Cooled  
Utilities Req’d: 120V/1PH, 5.8A; 3/8" CW, (2) 3/4" IW  
  
See plans for location and placement of item with reference to adjoining equipment.  
Furnish and set in place per manufacturer’s standard specifications and the following:  
1. Set in place in location as shown on drawings.  
2. Unit shall be all stainless steel construction.  
3. Coordinate the connection between ice maker and provide a Water Filtration System.  
4. Install ice maker under of Item #\_\_\_\_\_, Bar Top and Die, coordinate proper installation.  
5. Ice maker shall produce flaked ice.  
6. Provide bin with 110 lbs. ice storage capacity.  
7. Provide 6" stainless steel legs.  
8. Provide slide up and in bin door.  
9. Must meet all applicable governmental, and local laws, rules, regulations, and codes.