ITEM #: UNDERCOUNTER PLATE WARMER  
Quantity: One (1)  
Manufacturer: Custom Fabrication  
Model No.: Stainless Steel  
Pertinent Data: See Plans, Drawing #FS  
Utilities Req’d: 120V/1PH, 20.0A  
  
See plans for location and placement of item with reference to adjoining equipment.  
Fabricate and set in place per plans, details, and the following:  
1. Standard fabrication Drawing #FSX.X, Detail #???.  
2. Set in place in location as shown on drawings.  
3. Size and configuration as shown on drawings.  
4. Provide Chromalox Silicone Laminated Heater blanket on the top sides and bottom of the Cabinet.  
5. Equip the unit with sliding glass cabinet doors with integrally formed full length door pull and intermediate shelves.  
6. Provide Thermostatic Temperature Controls for the Chromalox Silicone Laminated Heater blanket.  
7. Coordinate installation and fabrication with Item #, Service Pass Counter with Heated Cabinets and Sliding Doors.  
8. Fabricate and install per NSF Standard 2, complete drawings, schedules, elevations, and details.   
9. All finished edges shall be #7 mirrored polish finish.  
10. Provide shop drawings for approval prior to fabrication.  
11. Must meet all applicable federal, state, and local laws, rules, regulations, and codes