ITEM #: UNDERCOUNTER REFRIGERATOR WITH DOORS  
Quantity: One (1)  
Manufacturer: Custom Fabrication  
Model No.: Stainless Steel  
Pertinent Data: See Plans Drawing #FS  
Utilities Req’d: 120V/1PH; 8.0A; 1” IW  
  
See plans for location and placement of item with reference to adjoining equipment.   
Fabricate and set in place per plans, details, and the following:  
1. Standard fabrication Drawing #FSX.X, Detail #32.  
2. Set in place in location as shown on drawings.  
3. Size and configuration as shown on drawings.  
4. Provide unit with heavy duty door track, to be tested to 115Kg.  
5. Provide unit with safety grip handles.  
6. Coordinate installation into Item #, Cold Preparation Counter With Sink.  
7. Condensing unit to be located where shown on drawings, mounted on a pull out tray. Unit is to consist of 1/3 HP compressor and all components necessary for a fully functioning system.  
8. Provide one piece, self-adjusting, magnetic gaskets.  
9. Provide 1” diameter NSF brass drain.  
10. Provide digital thermometer, to be fully integrated with the HACCP Compliant data collection system per General Conditions 2.31.  
11. Fabricate and install per NSF Standard 2, complete drawings, schedules, elevations, and details.  
12. All refrigeration components are to meet NSF 7 requirements.  
13. Provide shop drawings for approval prior to fabrication.  
14. Must meet all applicable federal, state, and local laws, rules, regulations, and codes.