ITEM #: UNDERCOUNTER REFRIGERATOR  
Quantity: One (1)  
Manufacturer: True Food Service Equipment  
Model No.: TUC-48-ADA-HC  
Pertinent Data: ---  
Utilities Req'd: 120V/1PH, 3.0A  
  
See plans for location and placement of item with reference to adjoining equipment.  
Furnish and set in place per manufacturer's standard specifications and the following:  
1. Set in place in location as shown on drawings.  
2. Provide unit with low profile casters.   
3. Provide unit with two (2) heavy duty stainless steel exterior doors.  
4. Provide each door fitted with a 12" long recessed handle that is foamed-in-place with a sheet metal interlock to ensure permanent attachment.  
5. Provide a positive seal self-closing doors with 90° stay open feature.  
6. Coordinate installation under Item #  
7. Provide low profile casters for an overall height of 31-7/8".   
8. Provide unit with heavy duty cord and plug, coordinate NEMA configuration with electrical contractor.  
9. Must meet all applicable federal, state, and local laws, rules, regulations, and codes.