ITEM #: UNDERCOUNTER REFRIGERATOR  
Quantity: One (1)  
Manufacturer: True Food Service Equipment   
Model No.: TUC-48G-ADA-HC  
Pertinent Data: Self-Contained  
Utilities Req’d: 120V/1PH; 3.0A

See plans for location and placement of item with reference to adjoining equipment.   
Furnish and set in place per manufacturer’s standard specifications and the following:  
1. Set in place in location as shown on drawings.  
2. Provide “Low-E”, double pane thermal glass assembly with extruded aluminum frames.   
3. Provide four (4) low profile heavy duty swivel casters two (2) with brakes for a total height of 31-7/8”.  
4. Provide heavy-duty cord and plug.  
5. Provide doors fitted with 12" (305 mm) long recessed handle that is foamed-in-place with a sheet metal interlock to ensure permanent attachment.  
6. Must meet all applicable federal, state, and local laws, rules, regulations, and codes.