ITEM #: UTENSIL WASHER  
Quantity: One (1)  
Manufacturer: Champion  
Model No.: PP-12-PT  
Pertinent Data: ---  
Utilities Req’d: 208V/3PH; 71.0A; 3/4” HW; 1-1/4” IW  
  
See plans for location and placement of item with reference to adjoining equipment.   
Furnish and set-in place per manufacturer’s standard specifications and the following:  
1. Set in place in location as shown on drawings.  
2. Dish machine shall provide for front service, all services must be accessible from the front of the unit, owner provided detergent dispenser shall be mounted in front.  
3. Provide external rinse hose and spray gun.  
4. Provide self-contained water heating.  
5. Provide moisture resistant control gauges.  
6. Provide recirculating wash water.  
7. Provide left to right operation.  
8. Provide adjustable wash and rinse cycles.  
9. Provide removable dual filtration system.  
10. Equip unit with electric heat.  
11. Provide unit with precision engineered spray patterns.  
12. Provide unit with Digital Control and Information Center.  
13. Provide two doors lift-up door type, single control handle. Counter balanced with self-lubricating guides, stainless steel cables on nylon rollers with cable guards to ensure tracking. Doors are interlocked with limit switch to prevent machine operation while doors are open. Door construction: 16-gauge, stainless steel.  
14. Provide shop drawings for approval prior to fabrication.  
15. Must meet all applicable federal, state, and local laws, rules, regulations, and codes.