ITEM #: VACUUM PACKAGIING MACHINE  
Quantity: One (1)  
Manufacturer: Sipromatic  
Model No.: 450-T  
Pertinent Data: Mobile  
Utilities Req’d: 120V/1PH; 6.5A  
  
See plans for location and placement of item with reference to adjoining equipment.   
Furnish and set in place per manufacturer’s standard specifications and the following:  
1. Set in place in location as shown on drawings.  
2. Provide counter top models with stainless steel housing and single chamber.  
3. Provide powerful, high quality 20 m3/h Busch pump and vacuum dial gauge.  
4. Provide single stainless steel 27.5” x 20” x 8” high chamber with vacuum intervals of 1 to 99 seconds.  
5. Provide two (2) 19.1” seal bars with high integrity double sealing.  
6. Provide simple to operate electronic touch pad controls.  
7. Provide gas flush for the addition of an anaerobic gas mixture and/or pillow pack seal.  
8. Provide heavy-duty cord and plug.  
9. Coordinate installation under Item #, Cold Preparation Table with Sink.  
10. Provide unit on four (4) 2” heavy-duty, non-marking casters, two (2) with brakes.  
11. Must meet all applicable federal, state, and local laws, rules, regulations, and codes.