ITEM #: VEGETABLE WASHER  
Quantity: One (1)  
Manufacturer: Nilma  
Model No.: ATIR I  
Pertinent Data: Tilting  
Utilities Req’d: 208V/3PH; 6.6A; 1” CW, 2” IW  
  
See plans for location and placement of item with reference to adjoining equipment.   
Furnish and set in place per manufacturer’s standard specifications and the following:  
1. Set in place in location as shown on drawings.  
2. Size and configuration as shown on drawings.  
3. Provide washing intensity adjusting control.  
4. Equip unit with water discharge adjusting control.  
5. Provide rotating water inlet faucet.  
6. Equip unit with an easy to inspect and clean washing basin.  
7. Unit shall be equipped with a hydraulic device for automatic product unloading.  
8. Unit construction shall be entirely stainless steel.  
9. Provide adjustable feet.  
10. Equip unit with a pump protection guard.  
11. Provide a trolley for vegetable transportation made of made of 18/10 stainless steel with four castors and removable basket made of white plasticized steel.  
12. Must meet all applicable federal, state, and local laws, rules, regulations, and codes.