ITEM #: VENTLESS EXHAUST HOOD  
Quantity: One (1)  
Manufacturer: Rational  
Model No.: 60.76.178  
Pertinent Data: UL Listed  
Utilities Req'd: 120V/1PH, 1.4A (light and fan), NEMA 5-15P; 415 CFM Extraction  
  
See plans for location and placement of item with reference to adjoining equipment.  
Furnish and set in place per manufacturer’s standard specifications and the following:  
1. Set in place in location as shown on drawings  
2. UltraVent® Plus Ventless Recirculating Condensation Hood, with HEPA filter for smoke capture, filters smoke, for single or Combi-Duo, for 6- and 10-full size (electric), 6' cord  
3. Provide unit with any and all installation kits to ensure a perfect fit onto Item #\_\_\_\_, Double Combi Oven.  
4. Must meet all applicable federal, state, and local laws, rules, regulations, and codes.