ITEM #: VENTLESS EXHAUST SYSTEM  
Quantity: One (1)  
Manufacturer: Rational  
Model No.: 60.76.179  
Pertinent Data:   
Utilities Req’d: 120V/1PH, 1.42A; 415 CFM Exhaust  
  
See plans for location and placement of item with reference to adjoining equipment.  
Furnish and set in place per manufacturer’s standard specifications and the following:  
1. Set in place in location as shown on drawings.  
2. Size and configuration as shown on drawings.  
3. Assembly to consist of one (1) section, 33-5/8”" long x 38-1/4" wide x 12-3/8" high, unit shall weigh 146 pounds. Construction to be a minimum of 18 gauge, 300 series stainless-steel with No. 4 finish.  
4. Unit shall be mounted directly onto Item #\_\_\_\_\_\_\_\_, Combi Oven.  
5. Provide Intelligent power control with automatic, continuously variable adjustment of the extraction power to the quantity of steam emitted.  
6. Unit shall automatically boosts extraction rate when cooking cabinet door is opened.  
7. Equip unit to eliminates lingering steam and vapours. These are extracted and condensed in the hood.  
8. Unit shall be easy to install and retrofit.  
9. Provide Issue of service notifications on the display of the iCombi Pro and iCombi Classic.  
10. Equip with adjustment of maximum extraction power on the display.  
11. Provide easy to clean baffle plate, dishwasher safe.  
12. Must meet all applicable federal, state, and local laws, rules, regulations, and codes.