ITEM #: VERTICAL CUTTER / MIXER  
Quantity: One (1)  
Manufacturer: Hobart  
Model No.: HCM450  
Pertinent Data: ---  
Utilities Req’d: 208V/3PH; 30.0A  
  
See plans for location and placement of item with reference to adjoining equipment.   
Furnish and set in place per manufacturer’s standard specifications and the following:  
1. Set in place in location as shown on drawings.  
2. Size and configuration as shown on drawings.  
3. Equip unit with a 45-quart capacity stainless steel bowl with pouring lip.  
4. Construct unit with a durable steel base with epoxy enamel finish.  
5. Unit shall be equipped with electromechanical safety interlocks, and Start/Stop push button switches.  
6. Provide the unit with a 5-minute timer with “Hold” and “Jog” settings.  
7. Equip the unit with a counterbalanced clear Lexan7 polycarbonate bowl cover with stainless steel support bar.  
8. Provide the unit with a bowl tilt lever which allows bowl to tilt to a 90-degree angle for easy pouring and removal of product.  
9. Provide a stainless steel mixing baffle with pour-through center shaft which will be manually operated to move products continually into the shaft blades, built-in bowl cover scraper allows for easy viewing of product, and pour-through center shaft permits addition of liquid products with the cover closed.  
10. Unit shall include a 2 Blade Cut/Mix Knife, a Knead/Mix Attachment, and a Polypropylene Strainer Basket.  
11. Provide with a 6’ heavy-duty cord and plug, coordinate NEMA configuration with Electrical Contractor.  
12. Must meet all applicable federal, state, and local laws, rules, regulations, and codes.