ITEM #: WASTE OIL CONTAINMENT TANK  
Quantity: One (1)  
Manufacturer: Frontline International   
Model No.: 2478SQ-NA  
Pertinent Data: Indoor  
Utilities Req’d: 120V/1PH; 15.0A

See plans for location and placement of item with reference to adjoining equipment.   
Furnish and set in place per manufacturer’s standard specifications and the following:  
1. Set in place in location as shown on drawings.  
2. Size and configuration as shown on drawings.  
3. Provide heavy-gauge stainless steel exterior sides, bottom and legs.  
4. Unit shall be freestanding, 24 in. square x 85.5 in. height.  
5. Provide 6” high stainless steel legs.  
6. Unit shall have a tank capacity of 1100 Lb/150 Gal.  
7. Equip unit with a control panel with power indication or digital reader.  
8. Provide level indicators with safety overflow protection.  
9. Unit shall be suitable for Direct Plumbed, Remote Plumbed or Caddy systems.  
10. Provide unit with INS-Kit for indoor installation.  
11. Unit shall be UL, UL Sanitation Listed.  
12. Must meet all applicable federal, state, and local laws, rules, regulations, and codes.