ITEM #: WASTE OIL CONTAINMENT TANK  
Quantity: One (1)  
Manufacturer: Frontline International   
Model No.: 4280-NA  
Pertinent Data: Indoor  
Utilities Req’d: 120V/1PH; 15.0A

See plans for location and placement of item with reference to adjoining equipment.   
Furnish and set in place per manufacturer’s standard specifications and the following:  
1. Set in place in location as shown on drawings.  
2. Size and configuration as shown on drawings.  
3. Provide heavy-gauge aluminum exterior.  
4. Unit shall be freestanding, 42 in. diameter x 80 in. height.  
5. Provide remote located control panel with power indication.  
6. Unit shall have a tank capacity of 2650 Lb/353 Gal.  
7. Provide level indicators with safety overflow protection.  
8. Unit shall be suitable for Direct Plumbed, Remote Plumbed or Caddy systems.  
9. Provide unit with INS-Kit for indoor installation.  
10. Unit shall be UL, UL Sanitation Listed.  
11. Must meet all applicable federal, state, and local laws, rules, regulations, and codes.