ITEM #: WASTE OIL CONTAINMENT TANK  
Quantity: One (1)  
Manufacturer: Frontline  
Model No.: 2478SQ-NA-DP  
Pertinent Data: 1100 Pounds  
Utilities Req’d: 120V/1PH; 15.0A  
  
See plans for location and placement of item with reference to adjoining equipment.  
Furnish and set in place per manufacturer’s standard specifications and the following:  
1. Set in place in location as shown on drawings.  
2. Size and configuration as shown on drawings.  
3. Provide heavy-gauge stainless-steel exterior sides, bottom and legs.  
4. Unit shall be freestanding, 24 in. square x 85.5 in. height.  
5. Provide 6" high stainless-steel legs.  
6. Unit shall have a tank capacity of 1,100 pounds/150 gallons.  
7. Equip unit with a control panel with power indication or digital reader.  
8. Provide level indicators with safety overflow protection.  
9. Unit shall be suitable for Direct-Plumbed, Remote-Plumbed or Caddy systems.  
10. Unit shall be UL, UL Sanitation Listed.  
11. Must meet all applicable federal, state, and local laws, rules, regulations, and codes.