ITEM #: WATER AND ICE STATION  
Quantity: One (1)  
Manufacturer: Delfield  
Model No.: 204P  
Pertinent Data: 45 LB Capacity  
Utilities Req’d: 1/2" CW; (2) 1" IW  
  
See plans for location and placement of item with reference to adjoining equipment.  
Furnish and set in place per manufacturer’s standard specifications and the following:  
1. Set in place in location as shown on drawings.  
2. Size and configuration as shown on drawings.  
3. Coordinate installation into Item #, Work Counter with Sink.  
4. Provide unit with a pitcher filler.  
5. Provide unit with chrome plated wire strainer.  
6. Provide top with 20-gauge stainless steel with die stamped drain opening.  
7. Provide 20-gauge stainless steel top with raised die stamped opening.  
8. Provide one-piece stainless steel lift off cover with handle.  
9. Provide 45-pound capacity ice chest.  
10. Provide factory applied gasket.  
11. Unit must be NSF Certified.  
12. Must meet all applicable federal, state, and local laws, rules, regulations, and codes.