ITEM #: WATER CHILLER  
Quantity: One (1)  
Manufacturer: Perfection  
Model No.: RA-34 RECIRCULATING  
Pertinent Data: Water Cooled, Self-Contained  
Utilities Req’d: 208V/1PH; 10.95A; 1/2” Chilled Water Supply, 1/2” Chilled Water Return

See plans for location and placement of item with reference to adjoining equipment.   
Furnish and set in place per manufacturer’s standard specifications and the following:  
1. Set in place in location as shown on drawings.  
2. Size and configuration as shown on drawings.  
3. Unit shall be provided with stable water conditions no rise and fall in water temperature,  
4. Provide unit with UltraChill Technology.  
5. Provide the recirculating feature to allow flexibility to serve multiple units.  
6. Equip the unit with a maximum line run of 500 foot.  
7. Coordinate installation with Item #, Water Meter.  
8. Unit shall be ceiling mounted and the General Contractor shall be responsible for supplying ceiling supports.  
9. Must meet all applicable federal, state, and local laws, rules, regulations, and codes.