ITEM #: WATER METER  
Quantity: One (1)  
Manufacturer: Gemini KB Systems  
Model No.: SAMM220  
Pertinent Data: ---  
Utilities Req’d: 3/4” HW, 3/4” CW

See plans for location and placement of item with reference to adjoining equipment.   
Furnish and set in place per manufacturer’s standard specifications and the following:  
1. Set in place in location as shown on drawings.  
2. Size and configuration as shown on drawings.  
3. Unit shall be wall mounted unit, 60” above floor level.  
4. Provide unit dimensions: W 7” X H 11” X D 6”.  
5. Units incoming water pressure should be regulated from 30psi minimum to 80psi maximum.  
6. Equip the unit with an outlet of 1/2” water line connection.  
9. Provide a notched wheel for setting dosing amount on graduated dial (1# to 220#).  
10. Equip unit with an Emergency cut off lever.  
11. Provide a water temperature gauge.  
12. Unit shall be equipped with a dosing start lever.  
13. Equip unit with a manual temperature mixing valve lever.  
14. Unit shall be supplied with 8’ water hose line with swan neck connection for hanging to mixing bowl.  
15. Must meet all applicable federal, state, and local laws, rules, regulations, and codes.