ITEM #: WINE REFRIGERATOR  
Quantity: One (1)  
Manufacturer: True  
Model No.: TR-30DZW-L-SG-A  
Pertinent Data: Single Section, Self-Contained  
Utilities Req’d: 120V/1PH; 1.2A

See plans for location and placement of item with reference to adjoining equipment.   
Furnish and set in place per manufacturer’s standard specifications and the following:  
1. Set in place in location as shown on drawings.  
2. Provide 300 series stainless steel exterior, and interior.  
3. Provide a low-E, double pane, UV tinted glass door with stainless steel door frame with a 120° stay open feature.  
4. Provide heavy-duty cord and plug.  
5. Provide lift-up grill on top of the unit with toe kick.  
6. Provide 2 independent zones with dual evaporators that can be adjusted from 40°F (4.4°C) to 65°F (18.3°C).  
7. Equip unit with full extension wine racks with unfinished cherry fronts that cradle the wine and prevent vibration.  
8. Must meet all applicable federal, state, and local laws, rules, regulations, and codes.