ITEM #: WORKTOP FREEZER  
Quantity: One (1)  
Manufacturer: True Food Service Equipment   
Model No.: TWT-27F-HC  
Pertinent Data: Self-Contained  
Utilities Req’d: 120V/1PH; 2.3A

See plans for location and placement of item with reference to adjoining equipment.   
Furnish and set in place per manufacturer’s standard specifications and the following:  
1. Set in place in location as shown on drawings.  
2. Provide stainless steel door, front and sides on the exterior, and aluminum sides, wall and back on the interior.  
3. Provide four (4) 5” heavy duty swivel casters two (2) with brakes.  
4. Provide heavy-duty cord and plug.  
5. Provide door fitted with 12" (305 mm) long recessed handle that is foamed-in-place with a sheet metal interlock to ensure permanent attachment.  
6. Must meet all applicable federal, state, and local laws, rules, regulations, and codes.