ITEM #: 275 LBS. SPIRAL DOUGH MIXER  
Quantity: One (1)  
Manufacturer: Gemini KB Systems  
Model No.: GB-ME200  
Pertinent Data: Fixed Bowl  
Utilities Req’d: 208V/3PH; 48.0A

See plans for location and placement of item with reference to adjoining equipment.   
Furnish and set in place per manufacturer’s standard specifications and the following:  
1. Set in place in location as shown on drawings.  
2. Size and configuration as shown on drawings.  
3. Equip unit with solid sturdy construction.  
4. Unit shall be supplied with a bowl cover which prevents flour dust emissions during mix cycle.  
5. Provide separate spiral and bowl motors.  
6. Unit shall have a belt driven transmission for quiet operation.  
7. Equip the unit with oversize motors.  
8. Unit shall have optimum mixing for large or small batches of dough.  
9. Provide the unit to be low maintenance and high reliability.  
10. Must meet all applicable federal, state, and local laws, rules, regulations, and codes.